

**QR SERIES**

**HOW TO SETUP INTERNET REMOTE ACCESS VIA DMZ**


1. Go to Main Menu and go to Network



1. In Network Menu, Enable DHCP and make a note on the IP address.



1. Go to Port Configuration and make a note on port numbers




1. Login to your Router from a computer.
2. Find DMZ setting in the Router.

You can call your Router support or your ISP

Or you can Google: Where is DMZ setting in Netgear Router (example)

1. Enable DMZ for the IP address of the DVR


This an example of enabling DMZ in Frontier Router.

1. 
2. From a computer on the same network as the DVR, go to [www.canyouseeme.org](http://www.canyouseeme.org)

Your IP is your Internet IP address.

Port to check: 85 (web port as listed above) – Check port – Success

Then check one more port: 9000 (client port)



1. If both ports are success, then you can use the IP address listed in canyouseeme to remote access your system from Phone or Computer.
2. Example how to set the QRVIEW App on your phone:

